* | multiply quaternion by a quaternion or vector
* | compound two robots
/ | divide quaternion by quaternion or scalar
about | summary of object size and type
angdiff | subtract 2 angles modulo 2pi
angvec2r | angle/vector to SO3
angvec2tr | angle/vector to SE3
Animate | record a graphical animation sequence
Arbotix | Interface to Arbotix robot controller
arrow3 | draw a 3D arrow (third party code)
bresenham | Bresenhan line drawing
Bug2 | bug navigation
ccodefunctionstring | Converts a symbolic expression into a C-code function
circle | compute/draw points on a circle
CodeGenerator | construct a robot specific code generator object
colnorm | columnwise norm of matrix
colorname | map color name to RGB
ctraj | Cartesian trajectory
delta2tr | differential motion vector to SE3
DHFactor | transform sequence to DH description
diff2 | elementwise diff
distancexform | compute distance transform
distributeblocks | Distribute blocks in Simulink block library
dockfigs | control figure docking with GUI
doesblockexist | Check existence of block in Simulink model
Dstar | D* planner
DXform | distance transform from map
e2h | Euclidean coordinates to homogeneous
edgelist | trace edge of a shape
eg_grav | joint 2 gravity load g(q2,q3)
eg_inertia | joint 1 inertia I(q1,q2)
eg_inertia22 | joint 2 inertia I(q3)
EKF | extended Kalman filter object
eul2jac | Euler angles to Jacobian
eul2r | Euler angles to SO3
eul2tr | Euler angles to SE3
gauss2d | Gaussian distribution in 2D
getprofilefunctionstats | [ funstats] = getprofilefunctionstats( pstats , desfun, varargin)
h2e | homogeneous coordinates to Euclidean
homline | create line from 2 points
homtrans | transform points
ishomog | true if argument is SE3
ishomog2 | true if argument is a 3x3 matrix
ismatrix | true if non scalar
isrot | true if argument is a SO3 matrix
isrot2 | true if argument is a 2x2 matrix
isvec | true if argument is a 3-vector
joy2tr | Update SE3 based on joystick input
joystick | Help for joystick interface mex file
joytest | demo of gaming joystick input
jsingu | find dependent joints
jtraj | joint space trajectory
Link | construct a general robot link object
lspb | 1D trapezoidal trajectory
Machine | Abstract robot interface class
makemap | build an occupancy grid
Map | point feature map object
mdl_3link3d | Simple 3DOF arm, no shoulder offset (DH, kine)
mdl_ball | high DOF chain that forms a ball
mdl_baxter | Baxter 2-arm robot (DH, kine)
mdl_coil | high DOF chain that forms a coil
mdl_Fanuc10L | Fanuc 10L (DH, kine)
mdl_hyper2d | 2D high DOF chain
mdl_hyper3d | 3D high DOF chain
mdl_irb140 | ABB IRB140 (DH, kine)
mdl_irb140_mdh | ABB IRB140 (MDH, kine)
mdl_jaco | Kinova Jaco arm (DH, kine)
mdl_KR5 | Kuka KR5 (DH, kine)
mdl_m16 | Fanuc M16 (DH, kine)
mdl_mico | Kinova Mico arm (DH, kine)
mdl_MotomanHP6 | Motoman HP6 (DH, kine)
mdl_nao | Alderabaran NAO arms and legs (DH, kine)
mdl_offset3 | simple 3 link model (DH, kine)
mdl_offset6 | simple 6 link model (DH, kine)
mdl_onelink | simple 1-link example (DH, kine)
mdl_p8 | Puma 560 on an XY base (DH, kine)
mdl_phantomx | PhantomX pincher 4DOF hobby arm (DH, kine)
mdl_planar1 | simple 1 link planar model (DH, kine)
mdl_planar2 | simple 2 link planar model (DH, kine)
mdl_planar3 | simple 3 link planar model (DH, kine)
mdl_puma560 | Puma 560 data (DH, kine, dyn)
mdl_puma560akb | Puma 560 data (MDH, kine, dyn)
mdl_quadrotor | simple quadrotor model
mdl_S4ABB2p8 | ABB S4 2.8 (DH, kine)
mdl_simple6 | simple 6 link model (DH, kine)
mdl_stanford | Stanford arm data (DH, kine, dyn)
mdl_stanford_mdh | Stanford arm data (MDH, kine, dyn)
mdl_twolink | simple 2-link example (DH, kine, dyn)
mdl_twolink_mdh | simple 2-link example (MDH, kine)
moveline | non-holonomic vehicle moving to a line
movepoint | non-holonomic vehicle moving to a point
movepose | non-holonomic vehicle moving to a pose
mstraj | multi-axis multi-segment trajectory
mtraj | multi-axis trajectory for arbitrary function
multidfprintf | printf extension
Navigation | Navigation superclass
numcols | number of columns in matrix
numrows | number of rows in matrix
oa2r | orientation and approach vector to SO3
oa2tr | orientation and approach vector to SE3
ParticleFilter | Monte Carlo estimator
peak | find peak in 1D signal
peak2 | find peak in 2D signal
PGraph | general purpose graph class
plot2 | plot trajectory
plot2 | Plot trajectories
plot_arrow | draw an arrow
plot_box | draw a box
plot_circle | draw a circle
plot_ellipse | draw an ellipse
plot_ellipse_inv | draw an ellipse
plot_homline | plot homogeneous line
plot_point | plot points
plot_poly | plot polygon
plot_sphere | draw a sphere
plot_vehicle | plot vehicle
plotbotopt |
plotp | plot points
plotp | Plot trajectories
polydiff | derivative of polynomial
Polygon | general purpose polygon class
Prismatic | construct a prismatic robot link object
PrismaticMDH | construct a prismatic robot link object
PRM | probabilistic roadmap planner
qplot | plot joint angle trajectories
Quaternion | constructor
Quaternion.interp | interpolate a quaternion
Quaternion.inv | invert a quaternion
Quaternion.norm | norm of a quaternion
Quaternion.plot | display a quaternion as a 3D rotation
Quaternion.unit | unitize a quaternion
r2t | SO3 to SE3
ramp | create linear ramp
randinit | initialize random number generator
RandomPath | driver for Vehicle object
RangeBearingSensor | "laser scanner" object
Revolute | construct a revolute robot link object
RevoluteMDH | construct a revolute robot link object
RobotArm | Connect SerialLink object to real robot
rot2 | SO2 rotation
rotx | SO3 for rotation about X-axis
roty | SO3 for rotation about Y-axis
rotz | SO3 for rotation about Z-axis
rpy2jac | RPY angles to Jacobian
rpy2r | roll/pitch/yaw angles to SO3
rpy2tr | roll/pitch/yaw angles to SE3
RRT | rapidly exploring random tree
rt2tr | (R,t) to SE3
rtbdemo | Serial-link manipulator demonstration
runscript | interactively step through a script
rvcpath | path to RVC install
se2 | create SE2
se3 | lift SE2 to SE3
Sensor | robot sensor superclass
SerialLink | construct a serial-link robot object
SerialLink.accel | forward dynamics
SerialLink.cinertia | Cartesian manipulator inertia matrix
SerialLink.coriolis | centripetal/coriolis torque
SerialLink.edit | interactively edit a robot object
SerialLink.fdyn | forward dynamics
SerialLink.fellipse | plot force ellipsoid
SerialLink.fkine | forward kinematics
SerialLink.friction | return joint friction torques
SerialLink.gravload | gravity loading
SerialLink.ikine | inverse kinematics (numeric)
SerialLink.ikine6s | inverse kinematics for 6-axis arm with sph.wrist
SerialLink.ikine_sym | inverse kinematics (symbolic)
SerialLink.inertia | manipulator inertia matrix
SerialLink.itorque | inertia torque
SerialLink.jacob0 | Jacobian in base coordinate frame
SerialLink.jacobn | Jacobian in end-effector coordinate frame
SerialLink.maniplty | compute manipulability
SerialLink.nofriction | return a robot object with no friction
SerialLink.perturb | return a robot object with perturbed parameters
SerialLink.plot | plot/animate robot
SerialLink.plot3d | plot/animate robot as solid model
SerialLink.rne | inverse dynamics
SerialLink.teach | drive a graphical robot
SerialLink.trchain | express as chain of SE(3) transforms
SerialLink.vellipse | plot velocity ellipsoid
simulinkext | Return file extension of Simulink block diagrams.
skew | vector to skew symmetric matrix
sl_bicycle | Simulink "bicycle model" of non-holonomic wheeled vehicle
sl_braitenberg | Simulink model a Braitenberg vehicle
sl_quadcopter | Simulink model of a flying quadcopter
symexpr2slblock | Create symbolic embedded MATLAB Function block
t2r | SE3 to SO3
tb_optparse | toolbox argument parser
tpoly | 1D polynomial trajectory
tr2angvec | SE3/SO3 to angle/vector form
tr2delta | SE3 to differential motion vector
tr2eul | SE3/SO3 to Euler angles
tr2jac | SE3 to Jacobian
tr2rpy | SE3/SO3 to roll/pitch/yaw angles
tr2rt | SE3 to (R,t)
tranimate | animate a coordinate frame
transl | set or extract the translational component of SE3
transl2 | set or extract the translational component of SE2
trchain | evaluate a series of transforms
trchain | chain of SE(3) transforms
trchain2 | chain of SE2 transforms
trinterp | interpolate SE3 s
tripleangle | graphical interactive three angle rotation
tripleangle | demonstrate angle sequences
trnorm | normalize SE3
trot2 | SO2 rotation
trotx | SE3 for rotation about X-axis
troty | SE3 for rotation about Y-axis
trotz | SE3 for rotation about Z-axis
trplot | plot SE3 as a coordinate frame
trplot2 | plot SE2 as a coordinate frame
trprint | print an SE3
trscale | SE3 for scale change
unit | unitize a vector
Vehicle | construct a mobile robot object
vex | skew symmetric matrix to vector
VREP | VREP interface class
VREP_arm | MATLAB mirror for VREP robot arm
VREP_camera | MATLAB mirror for VREP camera object
VREP_mirror | MATLAB mirror for VREP object
VREP_obj | MATLAB mirror for VREP object
walking | example of 4-legged walking robot
wtrans | transform wrench between frames
wtrans | transform a force/moment
xaxis | set x-axis scaling
xyzlabel | label axes x, y and z
yaxis | set y-axis scaling

- SE3: homogeneous transformation, a 4x4 matrix, in SE(3)
- SO3: rotation matrix, orthonormal 3x3 matrix, in SO(3)
- Functions of the form tr2XX will also accept an SE3 or SO3 as the argument
- SE2: homogeneous transformation, a 3x3 matrix, in SE(2)
- SO2: rotation matrix, orthonormal 2x2 matrix, in SO(2)
- Arbotix class in the folder robot/interfaces
- VREP classes are in the folder robot/interfaces/VREP
- located in the examples folder

Copyright © 1990-2011 Peter Corke