M-File Help: rpy2jac

M-File Help: rpy2jac | View code for rpy2jac

# rpy2jac

Jacobian from RPY angle rates to angular velocity

J = rpy2jac(eul) is a Jacobian matrix (3x3) that maps roll-pitch-yaw angle rates to angular velocity at the operating point RPY=[R,P,Y].

J = rpy2jac(R, p, y) as above but the roll-pitch-yaw angles are passed as separate arguments.

## Notes

- Used in the creation of an analytical Jacobian.

## See also

eul2jac, SerialLink.JACOBN

© 1990-2014 Peter Corke.