M-File Help: mdl_S4ABB2p8

M-File Help: mdl_S4ABB2p8 | View code for mdl_S4ABB2p8

# mdl_S4ABB2p8

Create kinematic model of ABB S4 2.8robot

MDL_S4ABB2p8 is a script creates the workspace variable R which describes the kinematic characteristics of an ABB S4 2.8 robot using standard DH conventions.

Also defines the workspace vector:

q0 | mastering position.

## Author

Wynand Swart, Mega Robots CC, P/O Box 8412, Pretoria, 0001, South Africa wynand.swart@gmail.com

## See also

SerialLink, mdl_fanuc10l, mdl_m16, mdl_motormanhp6, mdl_irb140, mdl_puma560

© 1990-2014 Peter Corke.